Limit cycle oscillation initiated l-h transition in globus-m tokamak [[1]](#footnote-1)\*)

DOI: 10.34854/ICPAF.2023.50.2023.1.1.034

1,2Belokurov A.A., 1Askinazi L.G., 1Gusev V.K., 1Kiselev E.O., 1Kurskiev G.S., 2Petrov A.V., 1Petrov Yu.V., 2Ponomarenko A.M., 1Tolstyakov S.Yu., 2Yashin A.Yu.

1Ioffe Institute, St.Petersburg, Russia, [belokurov@mail.ioffe.ru](mailto:belokurov@mail.ioffe.ru),  
2Peter the Great St. Petersburg Polytechnic University, St. Petersburg, Russia.

Studies of possibility of L-H transition, i.e. transition to improved confinement regime with suppressed turbulent transport (H-mode) is important for modern plasma physics and nuclear fusion. Turbulence is suppressed by highly inhomogeneous radial electric field [1].

Aside from L-H transition initiated by external Er perturbation, it is possible for internal processes in plasma which create such inhomogeneous Er self-consistently, e.g. zonal flows [2]. Zonal flows manifest itself as narrow radial layers of poloidal plasma rotation, which leads to generation of inhomogeneous Er on the border of adjacent layers; such Er could lead to turbulence suppresson. Effectiveness of suppression and possibility of L-H transition initiation depends on Er perturbation spatial and temporal parameters [3].

Intermediate state between L- and H-mode, or I-phase, characterized by presence of zonal flows in form of LCO (limit cycle oscillations) is observed on may tokamaks [2], including Globus-M tokamak [4]. Depending on observed LCO frequency, I-phase resulted in self-sustaining H-mode (with LCO frequency 6 kHz) or backwards transition to L-mode (with LCO frequency 8.5 kHz). This observation is in agreement with results of the studies of L-H transition initiation by varied Er of geodesic acoustic mode [3], which states that lesser frequency of varied Er is more effective for L-H transition initiation.

For experimental parameters of discharges with LCO in Globus-M tokamak there was created a numerical model which calculates density profile evolution with non-linear diffusion coefficient that considers turbulence suppression by inhomogeneous Er. Modeling results show that LCO with experimental Globus-M parameters could initiate L-H transition. Indeed lesser LCO frequency of 6 kHz leads to initiation of L-H transition, while higher LCO frequency of 8.5 kHz do not lead to L-H transition, which is in agreement with experiment.

Research was supported by RSF (project 18-72-10028).

References

1. Itoh S-I. and Itoh K. 1988 Phys. Rev. Lett. 60 2276
2. Schmitz L. et al 2017 Nucl. Fusion 57 025003
3. Askinazi L.G. et al 2017 Plasma Phys. Control. Fusion 59 014037
4. A.Yu. Yashin et al 2018 Nucl. Fusion 58 112009

1. \*) [abstracts of this report in Russian](http://www.fpl.gpi.ru/Zvenigorod/L/Mu/ru/BP-Belokurov.docx) [↑](#footnote-ref-1)